{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet2","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"merged":[[0,0,0,7],[1,0,1,2],[1,3,1,5],[1,6,1,7],[2,0,2,2],[2,3,2,5],[2,6,2,7],[3,0,7,0],[7,1,7,7],[8,0,12,0],[12,1,12,7],[13,0,13,2],[13,3,13,4],[13,5,13,7]],"flags":["formulas_cached_only"]}
[" 襄州区政府采购单位自行采购询价单（样表）"]
["采购单位（加盖公章）：",null,null,"实施计划备案号：",null,null,"2021年 月 日"]
["项目名称：洗手池、手术圆凳、脚凳",null,null,"联系人：周俊超",null,null,"电话：0710-2552959"]
["采          购                 需                求","品名","规格型号","配置或技术要求","数量","单价","合价（元）","供货地点"]
[null,"洗手池",null,"2人位洗手池，采用进口优质304不锈钢制造，不锈钢厚度≥1.2mm，采用拉丝技术处理，自带40L电热水器，可自由设定出水温度，洗手槽采用特制的坡度设计，可有效防止水溅到洗手池外，红外线感应水龙头，独立设置，不影响其他水嘴的使用，方便使用及维护。包安装 ",1,19166.67,19166.67,"襄州区人民医院指定位置"]
[null,"手术圆凳",null,"整体优质不锈钢制作，凳面采用3mm不锈钢板材，脚底装有防滑封头，凳面高低可调，调节顺滑",8,716.67,5733.33,"襄州区人民医院指定位置"]
[null,"踏脚凳",null,"整体优质不锈钢制作，上铺防滑垫，416mm*296mm*150mm",4,623.33,2493.33,"襄州区人民医院指定位置"]
[null,"预算总金额（大小写）:  贰万柒仟叁佰玖拾叁圆叁角叁分    27393.33元"]
["供\n应\n商           回\n复","品名","品牌规格型号","配置或技术要求","数量","单价","合价（元）","供货地点及周期"]
[null,"洗手池",{"$nulls":5},"襄州区人民医院指定位置"]
[null,"手术圆凳",{"$nulls":5},"襄州区人民医院指定位置"]
[null,"踏脚凳",{"$nulls":5},"襄州区人民医院指定位置"]
[null,"报价总金额（大小写）:"]
["供应商（加盖公章）：",null,null,"联系人：",null,"联系电话："]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}